There was no mention of any specific material to assign to the part. As such, I used 4140 steel as it is a common structural steel.

The 1kN force resulted in a 0.002186mm displacement, less than 100kPa stress primarily focused between the fixed hole and the bend of the arm, a yield strength of approximately 620MPa, and a strain value less than 2\*10^-7.